**BHA Robotics Academy**

**FTC Relic Recovery Phone Configuration**

**January 25, 2018**

**PHONE CONFIGURATION FILE: “0125”**

**Servo Controller 1 – AL026BYK**

* Port 1: “glimpse\_r\_servo”
* Port 2: “glimpse\_l\_servo”
* Port 3: “ball\_servo”

**Motor Controller 1 (AL00VWWY)**

* Port 1 (Tetrix Motor) = “right\_motor”
* Port 2 (Tetrix Motor) = “left\_motor”

**Motor Controller 0 (AL025TAU)**

* Port 1 (Tetrix Motor) = “ball\_lift”

**Device Interface Module**

* **I2Cdevices** 
  + Port 0 (MR\_Color Sensor) = “sensor\_color”
  + Port 1 (MR\_Gyro) = “sensor\_gyro”